OVERVIEW: The "Gamma-DE" (67N6E) radar is a mobile, long-range, active phased array radar 3D operating in the D-band (NATO).

DETAILS:  The "Gamma-DE" radar is designed to detect, identify, localize and track of wide range of targets, including high-altitude and low-observable air-launched targets in contested electronic environment and under natural noise.  It can track up to 200 targets.

Specifications:

Frequency: 		1.0-3.0 GHz (approx) (D Band)
Power output: 		 12.5 kW (average);  ?? MW (peak) 
PRF:			 unknown pps	
Accuracy:		 100m (range); 2 degrees  			
On/Off time:		unknown
Deploy/Stow Time	20 minutes from trailer
Max Detection Ranges:   216 nm (1m2 RCS)
			130 nm (0.1m2 RCS)
 			70nm (0.01m2 RCS)
 


NOTES: IOC: 1990s.  The 67N6E is the export version of the 67N6. The radar’s antenna and the turntable may be mounted on a semi-mobile 23.8m high tower (radar deployment platform 40V6M).   It can also be used for ATC duties.

SOURCES:  "Radar "Gamma-DE" (67N6E) Catalog Rosoboronexport." Accessed September 26, 2020. https://roe.ru/eng/catalog/air-defence-systems/radar-and-electro-optical-equipment-for-air-target-detection/%22Gamma-DE%22%20%2867N6E%29/ ; "67N6E «Gamma-D» - Radartutorial." Grundlagen Der Radartechnik. Accessed September 26, 2020. https://www.radartutorial.eu/19.kartei/02.surv/karte063.en.html; "Deconstructing Russian-made FCR and Search Radar of S-500, S-400 and S-300 SAM." Global Defense Corp. Last modified May 2, 2020. https://www.globaldefensecorp.com/2020/05/01/radar/.



