OVERVIEW: The P-18 radar (NATO name: SPOON REST D) is an mobile, 2-D early warning and target acquisition radar operating in the  "A" Band at 150-170 MHz.

DETAILS: The P-18 provides improved angular discrimination and ECCM capabilities over the earlier P-12.  It uses a single antenna for both transmission and reception. A complete system is usually composed of an antenna/shelter vehicle, a generator vehicle, and a secondary vehicle-mounted radar for IFF.  Weapons systems frequently associated with the P-18 include the SA-6 GAINFUL and the SA-3 GOA SAMs.

Specifications:

Frequency: 		150-170 MHz
Power output: 		500-540 W (average), 200kW (peak)
PRF:			360 Hz
Range Resolution:	926 m					
On/Off time:		3/5 min
Detection Ranges
  Fighter size aircraft
	500 m altitude:	60 km
 	10000m alt.:	270 km

NOTES: The P-18 entered service in 1970 and was widely exported.  VHF radars such as the P-18 remain important, as they can be better at detecting stealth aircraft than more recent, higher frequency radars.  Additionally, The operating frequencies of the P-18 allows the radar signal to diffract 5 - 10 % further around obstacles and the earth's curvature than higher frequency radars.


SOURCES: Janes Radar and Electronic Warfare Systems "P-12/P-18 series early-warning radars, 08 December 2004; "SPOON REST." GlobalSecurity.org - Reliable Security Information. Accessed February 28, 2015. http://www.globalsecurity.org/military/world/russia/spoon-rest.htm; Dr Carlo Kopp, Russian VHF counter stealth radars proliferate, www.ausairpower.net/SP/DT-Rus-VHF-Radar-2008.pdf ; P-18 Radar." Wikipedia, the Free Encyclopedia. Accessed March 2, 2015. http://en.wikipedia.org/wiki/P-18_radar ; "Radar Basics." Grundlagen Der Radartechnik. Accessed March 2, 2015. http://www.radartutorial.eu/19.kartei/karte909.en.html ; "Russian / PLA Low Band Surveillance Radar Systems (Counter LowObservable Technology Radars)." Air Power Australia. Accessed March 2, 2015. http://www.ausairpower.net/APA-Rus-Low-Band-Radars.html.
