OVERVIEW: The Type 347G aka TR-47C aka EFR-1 aka RICE BOWL radar is a shipboard, short-range, 2-D, air-search, fire control  radar operating in the I-Band (NATO)(IEEE: X-band).  

DETAILS:    The Type 347G radar is  in conjunction with the Type 76A dual-37mm automatic AAA.  It is a  coherent pulse doppler design  using an inverse Cassegrain antenna with twisted polarization. The radar features Moving Target Indicator/Detection and Anti-nodding, anti-clutter capability.


Specifications:

Frequency: 		8-10 GHz (I-Band)
Power output: 		150 kW (peak)
PRF:			unknown
Range Resolution:		unknown
Target speed:		unknown
Max Range, 2m2 RCS tgt:	6 nm
			
	

 NOTES: IOC  1987. Likely based on Italian RTN-20X.


SOURCES:  Friedman, The Naval Institute Guide to World Naval Weapons Systems (5th ed) 2005-06, pg. 223; "Type 347 Radar." LiquiSearch :: Finding the Past, Present & Future™. Accessed March 10, 2024. https://www.liquisearch.com/type_347_radar. ; 
"中国347G型（Rice Bowl）火控雷达_Type 347G (Rice Bowl) Fire-Control Radar_GlobalMil-环球防务网." GlobalMil-环球防务网-专业英文军事网站，专注武器装备资料和军事评论！. Accessed March 10, 2024. https://www.globalmil.com/military/navy/china/systems/fire_control/2010/0313/169.html.
