OVERVIEW: The YLC-2V is a road-mobile, medium/long-range 3-D guidance surveillance radar   operating in the E/F (NATO) band. 

DETAILS: YLC-2V radar is a mobile surveillance and medium/long-range surveillance radar that can be quickly deployed.  The system can be operated remotely and has been integrated onto a wheeled platform providing for high mobility. 

Specifications:

Frequency: 		 E/F Band (NATO), S Band (IEEE)))  
Power output: 		 5.5 kW(average); 85 kW (peak) 
PRF:			 unknown pps	
Range Resolution:	 	200 m (range), 0.3° azimuth 					
On/Off time:		 unknown
Deploy/Stow Time	 	40 min
Range:			270 nm

 
NOTES: IOC: 2014.  

SOURCES: "Ancile." Ancile. Accessed July 9, 2022. https://www.deagel.com/Sensor%20Systems/YLC-2V/a003065. ; "YLC-2 - Radartutorial." Grundlagen Der Radartechnik. Accessed July 9, 2022. https://www.radartutorial.eu/19.kartei/02.surv/karte032.en.html. ;"YLC-2V 3D Long Range Surveillance Radar." World Defense Review. Accessed July 9, 2022. https://worlddefensereview.blogspot.com/2012/07/ylc-2v-3d-long-range-surveillance-radar.html.