OVERVIEW: The Mys-M1E coastal radars are designed to detect and track surface ships and small-size high-speed targets in the open sea and littoral areas.  It operates in the "I" Band.

DETAILS: The Mys-M1E/MR-10M1E radars can be integrated into an automated data gathering and processing system. They are capable of automatic tracking of up to 89 targets at ranges of up to 32 miles; semiautomatic tracking of up to 10 targets.

The Radar "Mys-M1" systeme consist of four mobile units: a control post; a maintenance vehicle; and two power plants.
 
Specifications:

Frequency: 		I-Band
Power output: 		??
PRF:			??  pps
Range Resolution:	1% of range, 0.13 degrees bearing		
Runup time:		3.5 minutes
Set up time: 			

Detection Range:       108 nm (200 km) (large surface tgt., radar site 2,000 meter AGL)
			26 nm (48 km) (RCS=5m2, radar height 300m, tgt height 1 m)
			  
 
NOTES: The MR-10M1E is a stationary radar and Mys-M1E is the trailer-mounted version.

SOURCES: 
"Coastal Radar Mys-M1E | Catalog Rosoboronexport." Рособоронэкспорт | Официальный сайт. Accessed September 16, 2021. https://roe.ru/eng/catalog/naval-systems/stationary-electronic-systems/mys-m1e/ ; "Coastal Radar Mys-M1E | Catalog Rosoboronexport." Рособоронэкспорт | Официальный сайт. Accessed September 16, 2021. https://roe.ru/eng/catalog/naval-systems/stationary-electronic-systems/mys-m1e/. ; "ФОТО И МИР, PHOTOS AND THE WORLD. ВОЕННО-ПОЛИТИЧЕСКИЕ И ВОЕННО-ТЕХНИЧЕСКИЕ НОВОСТИ. MILITARY-POLITICAL AND MILITARY-TECHNICAL NEWS." ФОТО И МИР, PHOTOS AND THE WORLD. ВОЕННО-ПОЛИТИЧЕСКИЕ И ВОЕННО-ТЕХНИЧЕСКИЕ НОВОСТИ. MILITARY-POLITICAL AND MILITARY-TECHNICAL NEWS. Accessed September 16, 2021. https://foto-i-mir.ru/mys-m1e-rls/. ; "Mobile Coastal Radar System Mys-М1E." АО "Концерн "Гранит-Электрон". Accessed September 16, 2021. https://www.granit-electron.ru/en/products/military-products/sea-air-and-ground-based-radioelectronic-warfare-systems/mys-m1e.php.