OVERVIEW: The TRML-3D is a mobile, medium range, 3D phased array surveillance and target acquisition radar, operating in the NATO "G" (IEEE "C") Band.

DETAILS: The TRML-3D radar is a fully-coherent multi-mode phased array surveillance.    The 3D radar is capable of detecting, tracking, and classifying various types of airborne targets with a particular emphasis on small, fast low-flying aircraft, missiles and hovering helicopters. It can be deployed as a stand-alone radar or can be integrated into air defense networks in coordination with other radars and command control systems.   It has good ECCM capability. 

The TRML-3D  is designed to be rapidly deployable and have good cross-country mobility.  The vehicle uses a telescoping 12m tall antenna mast.


Specifications:

Frequency: 		4-6  GHz (G-Band)
Power output: 		?? kW (peak) 
PRF:			?? pps
Range Resolution:	?? degree azimuth		
Runup time:		??
Set up time: 		10 minutes

Detection Range:	107 nm

NOTES:  Transportable in a C-130.


SOURCES: "Ancile." Ancile. Accessed September 17, 2021. https://www.deagel.com/Tactical%20Vehicles/TRML-3D/a000467. ; "TRML-3D - Radartutorial." Grundlagen Der Radartechnik. Accessed September 17, 2021. https://www.radartutorial.eu/19.kartei/04.battle/karte008.en.html. ;"TRML-3D/32 - Mobile Air Surveillance and Defence Radar | HENSOLDT." Sensor Solutions | HENSOLDT. Accessed September 17, 2021. https://www.hensoldt.net/products/radar-iff-and-datalink/trml-3d/32/.
