OVERVIEW: The AN/TPS-32 is a transportable, long range, tactical 3-D radar operating in the E/F Band.

DETAILS:  The AN/TPS-32 was designed to operate as the 3D radar sensor for the marine tactical data system.  It also provides two positions for operators to vector interceptor aircraft to assigned targets. Automatic target detection, clutter elimination, and IFF are included. 

Specifications:

Frequency: 		  2.905-3.080 GHz (E/F Band (NATO), S Band (IEEE))
Power output: 		  unknown kW(average);  2.2 MW (peak) 
PRF:			  unknown Hz	
Range Accuracy:		 229 m (range),   0.5 degrees azimuth 					
On/Off time:		 unknown
Deploy/Stow Time	 120 minutes/  minutes
 
Detection Range  
Pd=90%, 1 m2 RCS:	  370 km
Pd=50%:			  556 km

  
NOTES:  Transportable by truck, helo or aircraft.  Initial IOC of the TPS-32 was in 1969. This system replaced the antiquated AN/MSQ-46 and AN/MSQ-77 Bomb Directing Central systems used during the Vietnam conflict to guide bombers to their target. It is also used by the Philippines with the Hawk air defense system.


SOURCES: "GROUND RADARS (Military Weapons)." What-when-how — In Depth Tutorials and Information. Accessed March 29, 2015. http://what-when-how.com/military-weapons/ground-radars-military-weapons/. ; Jane's Radar and Electronic Warfare Systems 2001-02, "AN/TPS-32 surveillance radar," 10 November 2000, pg. 3590-91 ; GlobalSecurity.org - Reliable Security Information. "AN/TPS-32." Accessed December 1, 2013. http://www.globalsecurity.org/military/systems/aircraft/systems/an-tps-32.htm
