OVERVIEW: The EMAK class icebreaker is a diesel-powered icebreaker.

DETAILS:  

 

NOTES: Displacement: 20,240 tons full load
       Speed: 19.5 knts
       Range: 40,000 nm @ 15 knts
       Complement: 118
       In Commission: 1973 
       Completed: 3 	  

SOURCES: Polmar, Norman, and Siegfried Breyer. Guide to the Soviet Navy. Annapolis, Md: Naval Institute Press, 1983, 321 ; 
