OVERVIEW: The HR-3000 RSRP aka HADR (Hughes Air Defense Radar) is a fixed, 3D phased array air defense radar operating in the NATO "F" (IEEE "S") Band.

DETAILS: 

Specifications:

Frequency: 		2.3-2.5 and 2.7-3.7  GHz (F-Band)
Power output: 		1.5 MW (peak); 32 kW (average) 
PRF:			60-1430 Hz
Resolution:		150m distance		
Runup time:		??
Set up time: 		N/A
Detection Range:	310 nm (instrumented); 98,000 feet

NOTES:  IOC 1985.  RSRP stands for "Radar South Region & Portugal".


SOURCES: "HADR - Radartutorial." Grundlagen Der Radartechnik. Accessed September 17, 2021. https://www.radartutorial.eu/19.kartei/02.surv/karte003.en.html ; "Germany Looks into Radar Picture Improvements." Defence News, Analysis, Data and Market Forecasting - Shephard Media. Last modified November 1, 2019. https://www.shephardmedia.com/news/digital-battlespace/german-look-radar-picture-improvements/.
