OVERVIEW: The Akwayafe-class is a 2 shaft, diesel-electric powered Coastal Patrol Craft.

DETAILS:  The Akwayafe-class is based on the Rodman-101 with a GRP (fiberglass) hull. Armament consists of a  two 12.7mm MG.  Electronics are a single Furuno navigation radar.

SPECIFICATIONS:
Displacement: 64 tons (full), 46 tons (standard)
Speed: 26 kts (max)
Engineering: 2 Detroit diesels; 2800 hp(m), 2 shafts
Range: 800 nm @ 18 kts
Endurance: several days
Complement: 9 crew, 16 max

NOTES: IOC: 2000. Units in class: JABANE (P105); AKWAYAFE (P106)


SOURCES: "JABANE Patrol Boats (2000) - Navy of Cameroon (Cameroon)." NAVYPEDIA - Fighting Ships of the World. Accessed May 1, 2022. https://old-navypedia.org/ships/cameroon/came_cf_jabane.htm. ; "Rodman 101." Rodman. Last modified February 14, 2022. https://rodman.es/en/producto/professional-nautical/patrol-boats/rodman-101/.