OVERVIEW:  The AN/APY-10 radar is an airborne, long-range, multimode surveillance radar operating in the NATO  "I"  (IEEE X ) band.


DETAILS: 

The AN/APY-10 can provide high resolution radar images in both overland and water modes. Available modes include color weather, synthetic aperture radar (SAR), inverse synthetic aperture radar (ISAR), short exposure periscope detection, and navigation.

In ISAR mode, the AN/APY-10 is capable of ultra-high resolution imaging modes for maritime and overland operations.

Specifications:

	Frequency:	8-10 GHz (I-band (NATO))
	PRF:		?? Khz (air-to-air)
	Pulse width:	?? µ sec (air-to-air)
	Power: 		?? kW (peak) 
	Scan Limits:	??    
	Range:		250 nm (instrumented)
				

NOTES:  IOC: 2012.  The AN/APY-10(I) purchased by India has an air-to-air mode.

SOURCES:  "AN/APY-10 - Radartutorial." Grundlagen Der Radartechnik. Accessed June 1, 2023. https://www.radartutorial.eu/19.kartei/08.airborne/karte062.en.html. ; Deagel. "AN/APY-10." Accessed June 1, 2023. https://www.deagel.com/Sensor%20Systems/ANAPY-10/a001212. ; Raytheon Intelligence and Space. "AN/APY-10 Maritime, Littoral and Overland Surveillance Radar." Just a Moment.. Accessed June 1, 2023. https://www.raytheonintelligenceandspace.com/what-we-do/decision-superiority/reconnaissance-systems/apy10.
