OVERVIEW: The PRV-11 radar (NATO name: SIDE NET) is a mobile, nodding height-finding radar operating in the E Band.

DETAILS: The PRV-11 is a mobile, van-mounted mobile radar. It features clutter and asyncronuous jamming protection.  Weapons systems associated with the P-37 include the SA-2 GUIDELINE, SA-3 GOA and SA-5 GAMMON. 

Specifications:

Frequency: 		2.7 GHz (E Band)
Power output: 		1.3 kW (average); 1.2 MW (peak)
PRF:			330, 730 Hz	
Range Resolution:	1.5 km (range) 					
On/Off time:		unknown
Deploy/Stow Time	unknown




 
NOTES: IOC 1962.  The SIDE NET is usually paired with a P-15, P-19 or P-15 M acquisition radar for missile guidance   


SOURCES: ""SIDE NET." GlobalSecurity.org - Reliable Security Information. Accessed March 16, 2015. http://www.globalsecurity.org/military/world/russia/side-net.htm ; "SIDE NET." GlobalSecurity.org - Reliable Security Information. Accessed March 16, 2015. http://www.globalsecurity.org/military/world/russia/side-net.htm ; "Radar Basics - PRW-11." Grundlagen Der Radartechnik. Accessed March 16, 2015. http://www.radartutorial.eu/19.kartei/karte915.fr.html.
