OVERVIEW: The Type 362 aka SR-47B aka ESR-1 radar is a shipboard, short-range, 2-D, air/surface search  radar operating in the I/J-Band (NATO).  

DETAILS: 
Specifications:

Frequency: 		  8-10 GHz (I Band (NATO), X Band (IEEE)) 
			
Power output: 		 ?? kW(est, acquisition radar)
PRF:			?? pps	
Range Accuracy:		  60 m (range); ?? m (altitude)
                         		 0.5° degrees azimuth					
On/Off time:		  unknown
 
Range, 2m2 RCS tgt: 	 	23 nm 
	0.1m2 tgt:	                     6.5 nm
			
			

 NOTES: IOC  1988. 


SOURCES: Friedman, The Naval Institute Guide to World Naval Weapons Systems (5th ed) 2005-06, pg. 218; 



 


