OVERVIEW: The AN/FPS-27 was a stationary, frequency diversity, long-range, 2-D radar operating in the E-band (NATO).

DETAILS:  The AN/FPS-27 used a vertically stacked beam to estimate the targets height. 

Specifications:

Frequency: 		2322-2670 MHz (E-Band (NATO) S-Band(IEEE)
Power output: 		30 KW (average);  15 MW (peak)
PRF:			  226-288 Hz	
Range Resolution:	 				
On/Off time:		unknown
Deploy/Stow Time	N/A
Max Range:		220 nm

		

NOTES: IOC: 1963.

SOURCES:    "AN/FPS-27 - Radartutorial." Grundlagen Der Radartechnik. Accessed April 27, 2020. https://www.radartutorial.eu/19.kartei/11.ancient/karte099.en.html ; "AN/FPS-27 Radar." Federation Of American Scientists – Science for a Safer, More Informed World. Accessed April 27, 2020. https://fas.org/nuke/guide/usa/airdef/an-fps-27.htm.
