OVERVIEW: The RSR-210N is a lightweight I-band 2D Naval Air/Sea Surveillance RADAR with several operation modes and optional IFF.  In operates in the  I-band (NATO).

DETAILS: The RSR-210N is designed for smaller naval and coastgurd vessels or as an auxiliary radar on larger vessels. Modes are surveillance, gun-fire support and helicopter control. The RSR-210N has a sPotted wave guide antenna and features a TWT, multi-channel (air and surface), fully coherent and a comprehensive ECM suite. Both channels can handle over 200 tracks. A three-channel pulse Doppler radar system, it is designed to perform efficiently in harsh environments and accurately detect small, fast-moving targets under weather, sea, and land conditions that cause clutter, or unwanted radar echoes.

Specifications
Frequency: 			I-band (NATO) / X-band
Power Output: 			8 kW
PRF:				prob depending on mode
Resolution azimuth:			 < 0.3 degrees
Resolution range:		 	< 10 m
Detection Ranges instrumented:
Surveillance air/surf = 		27 nm, Self-defence Air = 32 nm, Gun-fire Support = 13 nm, Helo guidance = 8 nm
Detection Range on 5m2 RCS fighter: 	25 nm


Notes: user include Norway.  Manufactered by Reutech Radar Systems, South Africa

SOURCES: "Reutech RSR-210N", including pdf. Oct22. "Reutech Radar Systems Develops Naval Air and Sea Surveillance Radar with Model-Based Design." MathWorks - Makers of MATLAB and Simulink - MATLAB & Simulink. Accessed March 12, 2024. https://nl.mathworks.com/company/user_stories/reutech-radar-systems-develops-naval-air-and-sea-surveillance-radar-with-model-based-design.html.