OVERVIEW: The Marconi S.266 is a fixed, 2D, Long-Range Air Search radar operating in the NATO "D" and "F" bands.

DETAILS: The S.266 is a long-range radar system using two radars in a back-to-back configuration.  Because it could not get height information, the a height finding radar such as the S.244 was usually associated with the system.  


Specifications:

Frequency			1.3 and 3.0 GHz (D and F band (NATO),  L and S Band (IEEE))
Power output: 			2.25 MW 
PRF:				?? pps
Range Resolution:		unknown
On/Off time: 			unknown min. 
Deploy/Stow time: 		N/A min
Maximum Range:			 km (range), km (altitude)
	  
 

NOTES: Used in NATO NADGE radar network.

SOURCES: "Marconi Radar History / Major Achievements of Marconi Radar." Marconi Radar History / MARCONI RADAR. Accessed October 5, 2021. https://marconiradarhistory.pbworks.com/w/page/36189315/Major%20achievements%20of%20Marconi%20Radar. ; Radar Pages. Accessed October 5, 2021. https://www.radarpages.co.uk/download/radar_g97.doc.
