OVERVIEW: The S-743D Martello radar is a transportable, long range 3D air surveillance radar, intended to monitor airspace.  It operates in the NATO "D" band.  

DETAILS: 

Specifications:

Frequency			1.43 GHz  (D band (NATO),  L Band (IEEE))
Power output: 			unknown (average); unknown (peak)
PRF:				unknown pps
Range Resolution:		unknown
On/Off time: 			unknown min. 
Deploy/Stow time: 		180-240 min (approx)
Maximum Range:			470 km (instrumented range), 100,000 feet (instrumented altitude)
				400 km v. 1m2 RCS target 
	  
NOTES:     

SOURCES: "743D Martello 3D Long Range Surveillance Radar." Marconi Radar History / MARCONI RADAR. Accessed December 8, 2018. https://marconiradarhistory.pbworks.com/f/743D%20Brochure.pdf ; "Marconi Radar History / Marconi Radar List." Marconi Radar History / MARCONI RADAR. Accessed December 8, 2018. https://marconiradarhistory.pbworks.com/w/page/53393225/Marconi%20radar%20list ; "Martello Series (S713/723, S743-D, S753)." Aerospace, Defense & Power Systems - Market Research, Intelligence & Consulting. Accessed December 8, 2018. https://www.forecastinternational.com/archive/disp_pdf.cfm?DACH_RECNO=693 ; "Radar Basics - Martello S 743." Grundlagen Der Radartechnik. Accessed December 8, 2018. http://www.radartutorial.eu/19.kartei/02.surv/karte009.en.html ; Zikidis (Maj, HAF), Konstantinos, Alexios Skondras (2nd Lt, HAF), and Charisios Tokas (2nd Lt, HAF). "Low Observable Principles, Stealth Aircraft and Anti-Stealth Technologies." .: SCIENPRESS LTD :. Accessed December 8, 2018. https://www.scienpress.com/Upload/JCM/Vol%204_1_9.pdf.


