OVERVIEW:  The SA-22 GREYHOUND (57E6 and 57E6E) is two-stage, solid fuel, low-to-high altitude, short range surface-to-air missile using command guidance.  It is equipped with a 20 kg HE fragmentation rod warhead.

DETAILS:  

The 57E6YE surface-to-air missile features a high acceleration short flight time at the boost phase.The missile uses an air-dynamic steering. 		


Specifications:
 
Weight: 		 71 kg 
Length: 		 3.16m 
Diameter: 		 0.09 m  (missile) 0.170m (booster)  
Wingspan: 		 ?? m 
Speed:			 knts (1300 m/s)
Range:			 0.8-9.7 nm (1-18 km)
Engagement Altitude:	 30-49,000 ft, (5-15000 m)   
Max target speed: 	 1943 knts (1000 m/s)
Kill probability:	 0.7-0.90 
Maneuverability:	unknown g	


NOTES:  IOC: 2012  

SOURCES: 
"2S6 Tunguska." Weaponsystems.net. Accessed July 31, 2021. https://weaponsystems.net/system/60-2S6+Tunguska. ; "Pantsir-S1 / S2 / SM Mobile Air Defense System." Thai Military and Asian Region. Last modified January 18, 2020. https://thaimilitaryandasianregion.wordpress.com/2015/10/30/pantsir-s1/. ; Pike, John. "57E6 / SA-22 GREYHOUND." GlobalSecurity.org. Last modified 6, 2020. https://www.globalsecurity.org/military/world/russia/57e6.htm.