OVERVIEW: The DABUR class PB is a two shaft, diesel-powered gun-armed patrol craft.

DETAILS:    

Specifications:

		Displacement: 45 tons full load
       		Speed: 29 knts
       		Range:  1200 nm @ 17 knts 
       		Complement: 6-9  
       		 
       		

NOTES: IOC 1970.  Thirty-one built.  Designed to be capable of overland transport.

SOURCES: Jane's Fighting Ships: 1987-88. Ihs Global, 1987, pg. 276;  
