OVERVIEW: The Type 341 aka RICE LAMP aka H/LJP-341A  radar is a  shipboard, short-range, 2-D, gun fire control radar operating in the I-Band (NATO).

DETAILS: The Type 341 is used to control 30 mm and 57 mm guns. The Type 341 radar can direct two guns simultaneously against a single target.

Specifications:

Frequency: 		  8-10 GHz (G Band (NATO), X Band (IEEE))
Power output: 		  ??kW(peak)
PRF:			?? pps
Pulse Width:		?? µs (some sources say 2 µs)	
Range Accuracy:		  ??					
On/Off time:		  unknown
 Range: 			 20 nm 
			 			

 NOTES: IOC  1984. The Type 341 is the first Chinese indigenously developed gun fire control radar.  THe land-based varient is known as the MW-5.

SOURCES:  Friedman, The Naval Institute Guide to World Naval Weapons Systems (5th ed) 2005-06, pg. 221-22; 

