OVERVIEW: The MAGADAN-class icebreaker is a 2-shaft, diesel-powered icebreaker.

DETAILS:   The MAGADAN-class icebreaker is a shallow-draft icebreaker built in Finland.  It is capable of breaking 1 meter thick ice at a speed of 2 knots.

Specifications: 

       Displacement: 5,560 tons full load
       Speed: 16.5 knts
       Range: 
       Complement: 
       
  	  
NOTES: IOC 1983. Three units in the class: MUDYUG, MAGADAN and DIKSON.


SOURCES: Jane's Fighting Ships: 1987-88. Ihs Global, 1987, pg. 646; CNO, "Understanding Soviet Naval Developments, 5th ed.", (April 1985), pg. 77
