OVERVIEW: The Type 354 aka MX-902 aka H/LJQ-354 aka  EYE SHIELD  radar is a  shipboard, medium-range, 2-D, low altitude air search radar operating in G-Band (NATO).

DETAILS: The EYE SHIELD can track four targets and designate two.

Specifications:

Frequency: 		  4-6 GHz (G Band (NATO), C Band (IEEE))
Power output: 		  500 kW(peak)
PRF:			400, 800 pps
Pulse Width:		4 µs (some sources say 2 µs)	
Range Accuracy:		  75 m (range); ?? m (altitude); 1.3° azimuth					
On/Off time:		  unknown
 Range, 10m2 RCS tgt: 	 50 nm 
			 			

 NOTES: IOC  1975. 

SOURCES:  Friedman, The Naval Institute Guide to World Naval Weapons Systems (5th ed) 2005-06, pg. 217; "Type 354 / MX-902, Námořní Rádiolokátor." Armedconflicts.com. Accessed March 13, 2024. https://www.armedconflicts.com/Type-354-MX-902-namorni-radiolokator-Eye-Shield-t39619

