OVERVIEW:  The Elta EL/M-2001Bis an airborne, short-range, pulse-Doppler, air-to-air/air-to-ground  ranging radar,  operating in the NATO  "I/J"  (IEEE X-K ) band.


DETAILS: 

 The Elta EL/M-2001B is a compact, lightweight, solid state dual mode radar, suitable for small aircraft.  It automatically acquires and tracks targets visible in the pilot's HUD, providing range information to the aircraft weapons control computer.  The radar is relatively unaffected by ground clutter.  

Specifications:

	Frequency:	8-20 GHz (I/J-band (NATO))
	PRF:		?? Khz (air-to-air)
	Pulse width:	?? µ sec (air-to-air)
	Power: 		?? kW (peak) 
	Scan Limits:	??   
	Range:		8 nm
				

NOTES:  IOC: 1976.  Used in some versions of the Mirage 5, Mig-21 and AMX aircraft.  Weighs under 50kg.

SOURCES:  Flight International, 7 April 1979, pg. 1071; Janes's Radar and Electronic Warfare Systems 2002-2003, "EL/M-2001B radar" dtd 09 November 2001
