OVERVIEW: The Jerong class gunboat is a 3-shaft, diesel-powered vessel for patrolling the EEZ, law enforcement and anti-piracy  missions.

DETAILS: The Jerong class  is a lighter variant of the Lurssen FPB 45 class. A small RHIB can be launched with it's small crane.  Armament includes a Bofors 57mm/70 Mk1 and a Bofors 40mm/70 gun. 
Sensors include a  I-band navigation radar, a WM28 Fire-Control radar and a laser range finder.

SPECIFICATIONS:
Displacement: 210 tons (standard), 255 tons (full)
Speed: 32 kts (max)
Engineering: 3 MTU MB 16V 538 TB90 diesels 9000hp 6.6MW sustained. 3 Shafts
Range: 2000 nm @ 14 kts
Endurance:
Complement: 36

NOTES: IOC: 1976.  Updated in 2021 with new main engines, propellors, generators gearboxes and shafts



SOURCES: "JERONG Fast Attack Craft (gun) (1976-1977)." NAVYPEDIA - Fighting Ships of the World. Accessed April 30, 2022. https://navypedia.org/ships/malaysia/mal_cf_jerong.htm. : "Jerung-class Gunboat." Wikipedia, the Free Encyclopedia. Last modified March 16, 2022. https://en.wikipedia.org/wiki/Jerung-class_gunboat. ; "Royal Malaysian Navy Completes Modernization of KD Jerong Fast Attack Craft." MilitaryLeak. Last modified April 17, 2021. https://militaryleak.com/2021/04/17/royal-malaysian-navy-completes-modernization-of-kd-jerong-fast-attack-craft/. ; "World Navies Today: Malaysia." Haze Gray & Underway - Naval History and Photography. Accessed April 30, 2022. https://www.hazegray.org/worldnav/asiapac/malaysia.htm#3.