OVERVIEW: The H/LJQ-364 aka Type 364  aka SR-64 aka Seagull-C radar is a shipboard, medium range, 2-D, air-search, targeting  radar operating in E/F-Band (NATO)(IEEE: S-band).  

DETAILS:    The Type 364 radar is used as the very low altitude rapid-response radar system of close-in antiship missile defense, primarily for CWIS and HQ-10 systems. It also likely has a secondary air search and SSM targeting abilities. It is capable of tracking over 20 targets.


Specifications:

Frequency: 		2-4 GHz ( E/F-Band)
Power output: 		100w (avg); 60kW (peak)
PRF:			unknown
Range Resolution:		unknown
Target speed:		unknown
Max Range, 2m2 RCS tgt:	40 nm;
	  0.1m2 RCS tgt:	6.5 nm 		
	

 NOTES: IOC  1993. Improved version of the Type 360.


SOURCES: Jane's Radar and Electronic Warfare Systems 2002-03, "30N6E/30N6E1 tracking radar" (09 November 2001); Friedman, The Naval Institute Guide to World Naval Weapons Systems (5th ed) 2005-06, pg. 219; "CPC Low Airspace Target Detection And Surveillance Radar System For Fire Control System." Quality Electro Optical Tracking System & Electro Optical Sensor System Factory from China. Accessed March 9, 2024. https://www.eo-irsystems.com/sale-7838637-cpc-low-airspace-target-detection-and-surveillance-radar-system-for-fire-control-system.html. ;"Type 364 Radar - Radartutorial." Grundlagen Der Radartechnik. Accessed March 9, 2024. https://www.radartutorial.eu/19.kartei/07.naval2/karte028.en.html